5. . A wire carrying 5.0 V is applied to a transformer. The primary coil has 5 turns and the secondary coil has 10 turns. What is the emf induced in the secondary coil? (A) 0.50 V (B) 5.0 V (C) 10 V (D) 50 V (E) 100 V