6. . What is the minimum incident angle for which the light will undergo total internal reflection in the plastic? (A) (B) (C) (D) 0Âº (E) 90Âº